MATERIAL SAFETY DATA SHEET

SHINING CRYSTALLIZER   CR-2

1. Product and manufacturer's identification.

Description of the product :  SHINING CRYSTALLIZER   CR-2.

Use : Shining crystallizer for marble and terrazzo pavements.

Manufacturer :	ABRASIVOS AGUILA S.A.

Riera de Palau, 13

08740-Sant Andreu de la Barca

Barcelona ( SPAIN )

Telephone.: +34 93 653 30 58	Fax.: +34 93 682 10 40

2. Composition/information about components.

Name	Concentration interval	Symbol	Risk fases

MAGNESIUM FLUOSILICATE  15-35 %	T	R 25/R 34/R 36/R 38

3. Identification of danger.

- Toxic for ingestion and external contact.

- A long exposure may cause irritation in mucous membrane and skin.

4. First aids.

Inhalation: Take the subject away from the contaminated zone and make him breath fresh air.

Contact with eyes : Wash immediately with water (15 min.), separating the eyelids. Consult with an ophthalmologist if the irritation continues.

Contact with skin : Take the dirty clothes away. Wash it with soap and water and rinse with clean water.

Ingestion : Drink ¼ l. of milk immediately, induce vomit and consult a physician.

Precaution : In case of poisoning or accident, it is recommendable to go to an emergency hospital service, since its ingestion may produce a serious hypocalcemia.

5. Measures of security against fires.

Non inflammable or explosive product.

6. Measures to take in case of accidental spill.

Spread some sand and recover the product in a container for a later destruction.

Avoid to pour out in the waste pipes, subterranean waters and drains.

Avoid the contact with the environment through filtrations or contact with the vegetation.

7. Handling and storage.

Air the premises during the handling. Use gloves and suitable protection.

Keep at temperature of no more than 30ºC, in a ventilated and dry place, protected from the sunlight, heat sources or focus of ignition.

8. Controls of exposure and personnel protection equipment.

Respiratory protection.	Not required for usual workings.

Protection of hands.	Use always protective gloves.

Protection of eyes.	Use protective glasses.

Protection of skin.	Change the dirty or sprikle clothes.

9. Chemical-physical properties.

Aspect : Pink liquid

Resistance to the temperature :	to the cold :       + 1ºC

Density : 1.100 gr/cc.	to the heat : + 45ºC

Soluble in water.	pH  :  2-3

10. Stability and reactivity.

The product does not discompose or change its stability if it is appropriately storaged.

11. Toxicological information.

Irritating for skin, eyes, mucous membrane and digestive tract.

12. Ecological information.

Do not pour out in drains or in the environment. It has to be eliminated in an authorized point of waste collection.

Toxic components for the environment : Magnesium Fluosilicate

13. Considerations concerning to the elimination.

Follow the valid regulations for the elimination of chemical wastes.

Avoid always to pour out in residual water pipes.

14. Information concerning to the transport.

This product is not considered as dangerous for transport.

15. Statutory information.

It has to be marked, according the present Spanish regulations :

ABRASIVOS AGUILA S.A.

SHINING CRYSTALLIZER   CR-2

SYMBOL OF TOXIC

SYMBOL OF CORROSIVE

It contains Magnesium Fluosilicate

Toxic for ingestion.	R 25

It causes burns.	R 34

It irritates eyes and skin.	R 36/38

Keep away from children.	S 2

Keep the container well closed.	S 7

Keep away from food, drinks and fooders.	S 13

Avoid the contact with eyes and skin.	S 24/25

In case of contact with eyes, wash immediately

with much water and go to the doctor.	S 26

In case of contact with skin, wash immediately with much water.	S 28.

In case of accident or unwell, go to the doctor immediately (show him the label if possible).	S 45

In case of ingestion go to a doctor immediately and show him the

label or the container.	S 46

16. Other informations.

Applications of the product :

Special product to be used after polishing the floor and for the maintenance of surfaces with an intense traffic. Do not use on metallic, aluminium, wood, ceramic and thermoplastic parts. On white marble, make previosuly a test of colour stability in non-visible zones. Keep into the original container.

INSTRUCTIONS FOR USE.

The surface has to be clean and dry.

Shake the container strongly before using.

Do not dilute or mix with other products.

Pour a little quantity of CR-2 on a surface of about 2 m2., spread the product uniformly with a shining machine equipped with a steel wool pad and rub until the product gets completely dry. Repeat the same so many times as necessary.

MATERIAL SAFETY DATA SHEET

SHINING CRYSTALLIZER   CR-3

1. Product and manufacturer's identification.

Description of the product :  SHINING CRYSTALLIZER   CR-3.

Use : Product for the regular maintenance of crystallization on marble and terrazzo pavements.

Company :	ABRASIVOS AGUILA S.A.

Riera de Palau, 13

08740-Sant Andreu de la Barca

Barcelona ( SPAIN )

Telephone.: +34 93 653 30 58	Fax.: +34 93 682 10 40

2. Composition/information about components.

Name	Concentration interval	Symbol	Risk fases

MAGNESIUM FLUOSILICATE  15-30 %	T	R 25

3. Identification of danger.

- Harmful for ingestion and external contact.

- A long exposure may cause irritation in mucous membrane and skin.

4. First aids.

Inhalation : Take the subject away from the contaminated zone and make him breath fresh air.

Contact with eyes : Wash immediately with water (15 min.), separating the eyelids. Consult with an ophthalmologist if the irritation continues.

Contact with skin : Take the dirty clothes away. Wash it with soap and water and rinse with clean water.

Ingestion : Rinse the mouth out. Consult with a doctor.

Precaution : In case of poisoning or accident, it is recommendable to go to an urgency hospital, since its ingestion can produce a serious hypocalcemia.

5. Measures of security against fires.

Non inflammable or explosive product.

6. Measures to take in case of accidental spill.

Spread some sand and recover the product in a container for a later destruction.

Avoid to pour out in the waste pipes, subterranean waters and drains.

Avoid the contact with the environment through filtrations or contact with the vegetation.

7. Handling and storage.

Air the premises during the handling. Use gloves and suitable protection.

Keep at temperature of no more than 30ºC, in a ventilated and dry place, protected from the sunlight, heat sources or focus of ignition.

8. Controls of exposure and personnel protection equipment.

Respiratory protection.	Not required for usual workings.

Protection of hands.	Use always protective gloves.

Protection of eyes.	Use protective glasses.

Protection of skin.	Change the dirty or sprikle clothes.

9. Chemical-physical properties.

Aspect : Yellow liquid.	Resistance to the temperature :

to the cold :       + 1ºC

Density : 1.000 gr/cc.	to the heat : + 45ºC

Soluble in water.	pH  :  2-3

10. Stability and reactivity.

The product does not discompose or change its stability if it is appropriately storaged.

11. Toxicological information.

Irritating for skin, eyes, mucous membrane and digestive tract.

12. Ecological information.

Do not pour out in drains or in the environment. It has to be eliminated in an authorized point of waste collection.

Toxic components for the environment : Fluosilicato de magnesio and Phosphoric acid.

13. Considerations concerning to the elimination.

Follow the valid regulations for the elimination of chemical wastes.

Avoid always to pour out in residual water pipes.

14. Information concerning to the transport.

This product is not considered as dangerous for transport.

15. Statutory information.

It has to be marked, according the present Spanish regulations :

ABRASIVOS AGUILA S.A.

SHINING CRYSTALLIZER   CR-3

SYMBOL OF HARMFUL

SYMBOL OF CORROSIVE

It contains Magnesium Fluosilicate .

Harmful for ingestion.	R 25

It causes burns.	R 35

It irritates eyes and skin.	R 36/38

Keep away from children.	S 2

Keep the container well closed.	S 7

Keep away from food, drinks and fooders.	S 13

Avoid the contact with eyes and skin.	S 24/25

In case of contact with eyes, wash immediately with much water

and go to the doctor.	S 26

In case of contact with skin, wash immediately with much water.	S 28.

In case of accident or unwell, go to the doctor immediately (show him the label if possible).	S 45

In case of ingestion go to a doctor immediately and show him the

label or the container.	S 46

16. Other informations.

Applications of the product :

Special product for the regular maintenance of business premises. Quick application product. Recommended for white colour marbles. Do not use on metallic, aluminium, wood, ceramic, and thermoplastic parts. Keep in the original container.

INSTRUCTIONS FOR USE.

The surface has to be clean and dry.

Shake the container strongly before using.

Do not dilute or mix with other products.

Pour a little quantity of CR-3 on a surface of about 2 m2., spread the product uniformly with a shining machine equipped with fine steel wool and rub until the product gets completely dry. Repeat the same so many times as necessary.

MATERIAL SAFETY DATA SHEET

SHINING CRYSTALLIZER   CR-5  "BLACK GRANITE GLASS"

1. Product and manufacturer's identification.

Description of the product :  SHINING CRYSTALLIZER   CR-5  "BLACK GRANITE GLASS"

Use : Shining crystallizer for dark granite pavements.

Company :	ABRASIVOS AGUILA S.A.

Riera de Palau, 13

08740-Sant Andreu de la Barca

Barcelona ( SPAIN )

Telephone.: +34 93 653 30 58	Fax.: +34 93 682 10 40

2. Composition/information about components.

According to the present Spanish regulations, this product does not contain any component of obligatory information.

3. Identification of danger.

- Harmful for ingestion and external contact.

- A long exposure may cause irritation in mucous membrane and skin.

4. First aids.

Inhalation : Take the subject away from the contaminated zone and make him breath fresh air.

Contact with eyes : Wash immediately with water (15 min.), separating the eyelids. Consult with an ophthalmologist if the irritation continues.

Contact with skin : Take the dirty clothes away. Wash it with soap and water and rinse with clean water.

Ingestion : Rinse the mouth out. Consult with a doctor.

5. Measures of security against fires.

Non inflammable or explosive product.

6. Measures to take in case of accidental spill.

Spread some sand and recover the product in a container for a later destruction.

Avoid to pour out in the waste pipes, subterranean waters and drains.

7. Handling and storage.

Air the premises during the handling. Use gloves and suitable protection.

Keep at temperature of no more than 30ºC, in a ventilated and dry place, protected from the sunlight, heat sources or focus of ignition.

8. Controls of exposure and personnel protection equipment.

Respiratory protection.	Not required for usual workings.

Protection of hands.	Use always protective gloves.

Protection of eyes.	Use protective glasses.

Protection of skin.	Change the dirty or sprikle clothes.

9. Chemical-physical properties.

Aspect : Dark grey / black liquid.	Resistance to the temperature :

to the cold :       + 1ºC

Density : 1.000 gr/cc.	to the heat : + 45ºC

Soluble in water.	pH  :  approx. 7.

10. Stability and reactivity.

The product does not discompose or change its stability if it is appropriately storaged.

11. Toxicological information.

Irritating for skin, eyes, mucous membrane and digestive tract.

12. Ecological information.

Do not pour out in drains or in the environment. It has to be eliminated in an authorized point of waste collection.

13. Considerations concerning to the elimination.

Follow the valid regulations for the elimination of chemical wastes.

Avoid always to pour out in residual water pipes.

14. Information concerning to the transport.

This product is not considered as dangerous for transport.

15. Statutory information.

According to the present Spanish regulations, no warning of risk is necessary on the label.

The product is not suitable for human consumption.

Harmful for ingestion.	R 22

Toxic for inhalation, ingestion and in contact with skin.	R 23/24/25

It causes burns.	R 34

It irritates eyes and skin.	R 36/38

Possibility of irreversible effects.	R 40

Possibility of sensitization in contact with skin.	R 43

Keep away from children.	S 2

Keep the container well closed.	S 7

Keep away from food, drinks and fooders.	S 13

Avoid the contact with eyes and skin.	S 24/25

In case of contact with eyes, wash immediately with much water

and go to the doctor.	S 26

In case of contact with skin, wash immediately with much water.	S 28.

In case of accident or unwell, go to the doctor immediately (show him the label if possible).	S 45

In case of ingestion go to a doctor immediately and show him the

label or the container.	S 46

16. Other informations.

Applications of the product :

For black granite floors.

Special product to be used after polishing the floor and shining with Grey Potea, and for maintenance of surfaces with an intense traffic in black and very dark granites. Do not use on metallic, aluminium, wood, and thermoplastic parts.

Keep in the original container.

INSTRUCTIONS FOR USE.

The surface has to be clean and dry.

Shake the container strongly before using.

Do not dilute or mix with other products.

Pour a little quantity of CR-5 on a surface of about 2 m2, spread the product uniformly with a shining machine equipped with fine steel wool and rub until the product gets completely dry. Repeat the same so many times as necessary.

MATERIAL SAFETY DATA SHEET

SHINING CRYSTALLIZER   CR-6 "LIGHT GRANITE GLASS"

1. Product and manufacturer's identification.

Description of the product :  SHINING CRYSTALLIZER   CR-6  "LIGHT GRANITE GLASS"

Use : Shining crystallizer for white and clear granite pavements.

Company :	ABRASIVOS AGUILA S.A.

Riera de Palau, 13

08740-Sant Andreu de la Barca

Barcelona ( SPAIN )

Telephone.: +34 93 653 30 58	Fax.: +34 93 682 10 40

2. Composition/information about components.

According to the present Spanish regulations, this product does not contain any component of obligatory information.

3. Identification of danger.

- Harmful for ingestion and external contact.

- A long exposure may cause irritation in mucous membrane and skin.

4. First aids.

Inhalation : Take the subject away from the contaminated zone and make him breath fresh air.

Contact with eyes : Wash immediately with water (15 min.), separating the eyelids. Consult with an ophthalmologist if the irritation continues.

Contact with skin : Take the dirty clothes away. Wash it with soap and water and rinse with clean water.

Ingestion : Rinse the mouth out. Consult with a doctor.

5. Measures of security against fires.

Non inflammable or explosive product.

6. Measures to take in case of accidental spill.

Spread some sand and recover the product in a container for a later destruction.

Avoid to pour out in the waste pipes, subterranean waters and drains.

7. Handling and storage.

Air the premises during the handling. Use gloves and suitable protection.

Keep at temperature of no more than 30ºC, in a ventilated and dry place, protected from the sunlight, heat sources or focus of ignition.

8. Controls of exposure and personnel protection equipment.

Respiratory protection.	Not required for usual workings.

Protection of hands.	Use always protective gloves.

Protection of eyes.	Use protective glasses.

Protection of skin.	Change the dirty or sprikle clothes.

9. Chemical-physical properties.

Aspect : White liquid.	Resistance to the temperature :	to the cold :   + 1ºC

Density : 1.000 gr/cc.	to the heat :   + 45ºC

Soluble in water.	pH  :  approx. 7.

10. Stability and reactivity.

The product does not discompose or change its stability if it is appropriately storaged.

11. Toxicological information.

Irritating for skin, eyes, mucous membrane and digestive tract.

12. Ecological information.

Do not pour out in drains or in the environment. It has to be eliminated in an authorized point of waste collection.

13. Considerations concerning to the elimination.

Follow the valid regulations for the elimination of chemical wastes.

Avoid always to pour out in residual water pipes.

14. Information concerning to the transport.

This product is not considered as dangerous for transport.

15. Statutory information.

According to the present Spanish regulations, no warning of risk is necessary on the label.

The product is not suitable for human consumption.

Harmful for ingestion.	R 22

Toxic for inhalation, ingestion and in contact with skin.	R 23/24/25

It causes burns.	R 34

It irritates eyes and skin.	R 36/38

Possibility of irreversible effects.	R 40

Possibility of sensitization in contact with skin.	R 43

Keep away from children.	S 2

Keep the container well closed.	S 7

Keep away from food, drinks and fooders.	S 13

Avoid the contact with eyes and skin.	S 24/25

In case of contact with eyes, wash immediately with much water

and go to the doctor.	S 26

In case of contact with skin, wash immediately with much water.	S 28.

In case of accident or unwell, go to the doctor immediately (show him the label if possible).	S 45

In case of ingestion go to a doctor immediately and show him the

label or the container.	S 46

16. Other informations.

Applications of the product :

For white and light granite floors.

Special product to be used after polishing the floor and shining with White Potea, and for maintenance of surfaces with an intense traffic in light colour, white, pink and several tonalities granites. Do not use on metallic, aluminium, wood, and thermoplastic parts.

Keep in the original container.

INSTRUCTIONS FOR USE.

The surface has to be clean and dry.

Shake the container strongly before using.

Do not dilute or mix with other products.

Pour a little quantity of CR-6 on a surface of about 2 m2, spread the product uniformly with a shining machine equipped with fine steel wool no. 0 and rub until the product gets completely dry and obtain the required shine.